[Common]
ModelName="EPSON PM-G820 (M)"
SEND_TI=SUPPORT
Resource=EP0NOE13.dll
LeverAlart=On
SendCommand=1,0
UseRes=0,14
JobNameCom=1

[HeadUty]
NozzleCheck=2
CleanHead=0

[Calibration]
DD5M3Offset=TRUE
CalibType=2,1,2
CItemNum=3
CItem1=9,0
CItem2=9,0
CItem3=9,0
CItemDef=5
